Bowen Ratio

The Bowen Ratio is defined as the ratio between the sensible heat and the latent heat :

where is the temperature of the water surface and is the temperature of the atmosphere in degrees Celsius. while are the vapour pressure of the water surface and of the atmosphere, is the atmospheric pressure in mb (millibar). The Bowen ratio is used among other applications for the energy budet of open lake evaporation.